**Manual of QPST Download Tool**

1. download the **QPST tools** from “tools.tar.bz2” and install it

2. Dowload the Build Images from below link

[Build images](https://cloudtron.smartron.com/index.php/s/X7TavAe4tbP9OiA)

1.2 Open QFIL from Start Menu like this: **Start-> QPST -> QFIL.**

**2. Software Download by using QFIL**


2.1 Run QFIL. If the phone is connected, the port will recognized automatically. If not, click the button s**elect Port”**.

Note : If userbuild is there in device then port will not be detected,get the device in edl(emergency downloader) mode.by using below command then USB port will be detected.


>>adb shell

>>reboot edl

**>>** press Power button + vol up + vol down key together till device vibrate.then connect device to PC .




**PORT Selection**




2.2 If any another programs except QFIL, the software will prompt you to close them. We suggest that you click the button **Configuration”** and select the option **reset After Download”**.


Select the option **Flat build** in **select build type”**.




Click the button Browser beside **select Programmer”** and choose the file **prog\_emmc\_firehose\_8976\_ddr.mbn** in the phone software folder, and Search Path will be filled automatically.




2.4 Click the button **Load XML”**, the dialog box will pop up twice to let you select the **rawprogram0\_unparse** and **patch0.xml.**





2.5 Finally, click the button **Download”**. Then the progress bar will be visible, and downloading begins.

2.6 Downloading finished as follows. (**Pay attention to the textbox Status**)



**Download Success**

